AT-ETX-2I-64E1T1

Bill of Materials

1. RAD products:

|  |  |
| --- | --- |
| ETX-2I-64E1T1 | 1 |
| RM-34 (for ATE-PIO-USB,ATE-MMUX,ETX-205A, ETX-2I-64E1T1, ATE-RELAY-BOX-4) | 7 |
| ETX-205A/AC/19/PTP | 2 |
| ETX-204A\_DTAG/H/AC/OAM/EXT with Ethernet Generator program | 1 |
| ATE-DXC-4-8 | 1 |

1. A.T.E. products:

|  |  |
| --- | --- |
| ATE-PIO-USB | 1 |
| ATE-RELAY-BOX-4 | 1 |
| ATE-MultiMux | 2 |

1. Cables:
   1. RAD cables:

|  |  |
| --- | --- |
| CBL-RJ45/D9/F/6FT | 2 |
| CBL-ETH/UTP/STR | 4 |
| CBL-MUSB-DB9F | 2 |
| CBL-MP-28 | 2 |
| CBL-USB-B | 1 |
| CBL-DB9F-DB9M-STR | 2 |
| CBL-MP-RJ45/CROSS/0.2M | 64 |
| CBL-RJ45/2BNC | 3 |
| BNC splitter T-type | 1 |

* 1. Specify cables:

|  |  |
| --- | --- |
| AT-ETX2i64E1T1/CBL01 | 1 |
| AT-ETX2i64E1T1/CBL02 | 2 |
| AT-ETX2i64E1T1/CBL03 | 1 |
| AT-ETX2i64E1T1/CBL04 | 2 |
| AT-ETX2i64E1T1/CBL05 | 4 |
| AT-ETX2i64E1T1/CBL06 | 2 |
| AT-ETX2i64E1T1/CBL07 | 1 |
| AT-ETX2i64E1T1/CBL08 | 1 |

1. Mechanic parts:

|  |  |
| --- | --- |
| Masad (width 19”) | 1 (height 32U) |
| Fixed Shelf | 3 |
| Removeable Shelf | 1 |

1. Test equipment
   1. PC’s card

|  |  |
| --- | --- |
| Ethernet card | 2 |

* 1. Movable equipment

|  |  |
| --- | --- |
| Barcode scanner | 1 |
| USB-4xRS232 | 2 |
| Scope with 2 CHs | 1 |

1. PC
   1. PC
   2. Screen
   3. Keyboard
   4. Mouse
2. Miscellaneous:
   1. 5-way long power cable 230v …...…..…… 2 units
   2. Extension power cable 230v ..………..…… 1 unit
   3. Multiple power socket ..…………………… 1 unit
   4. Mouse pad …………………………....…… 1 unit
   5. Anti static surface …………………….….…. 1 unit